CAN CONTROLLED AREA NETWORK

It has 2 formats

Standard format

Extended format

Standard format is 11 bit identifier

Extended format is 29 bit identifier