Properties of CAN

Prioritization of message

Guaranty of latency times

Configuration flexibility

System wide data consistency

Multicast reception